IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2026-06-03T12:45:50"
Preprocessor: "IfcOpenShell 0.8.5-1c5b825"
Originating system: "IfcOpenShell 0.8.5-1c5b825"

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "AssembleTile BIM Library"
  IFCSITE "Site"
    IFCBUILDING "Building"
      IFCBUILDINGSTOREY "Level 1"
        contains 1 element
          1 x IFCCOVERING | CEILING | names: "AssembleTile 600x600 Kant E — Eik" | material: layers "AssembleTile" ("PET-filt hvit 9mm — 100% resirkulert polyester" 9., "Eik (Quercus robur) — massivt tre" 21.) | property sets: Pset_AssembleTile

Property sets
  Pset_AssembleTile | properties | on 1 object (1 IFCCOVERING)
    AcousticClass_200mmGap = "Klasse B — αw ≈ 0.75-0.80" (IFCLABEL)
    AcousticClass_NoAirGap = "Klasse C — αw ≈ 0.60" (IFCLABEL)
    BackingMaterial = "PET-filt 9mm hvit, 100% resirkulert polyester" (IFCLABEL)
    CompatibleSystem = "T-24 24mm flansch — alle fabrikanter" (IFCLABEL)
    Demountable = TRUE (IFCBOOLEAN)
    Description = "Trespilepanel for T-24 systemhimling, 600x600mm Kant E, Eik" (IFCLABEL)
    EdgeType = "Kant E" (IFCLABEL)
    ExpectedLifetime_years = 50 (IFCINTEGER)
    FSCCertified = TRUE (IFCBOOLEAN)
    FireRating_Class = "D-s2,d0 / B-s1,d0 brannlakkert+Sandler II.12" (IFCLABEL)
    FireRating_Standard = "EN 13501-1:2019" (IFCLABEL)
    Manufacturer = "Assemble Monter AS" (IFCLABEL)
    NominalLength_mm = 600. (IFCREAL)
    NominalThickness_mm = 30. (IFCREAL)
    NominalWidth_mm = 600. (IFCREAL)
    PETPlateLength_mm = 592. (IFCREAL)
    PETPlateThickness_mm = 9. (IFCREAL)
    PETPlateWidth_mm = 592. (IFCREAL)
    ProductCode = "AT-600E-EIK" (IFCLABEL)
    ProductName = "AssembleTile" (IFCLABEL)
    SlattCount = 10 (IFCINTEGER)
    SlattGap_mm = 26. (IFCREAL)
    SlattHeight_mm = 21. (IFCREAL)
    SlattLength_mm = 574. (IFCREAL)
    SlattMaterial = "Eik (Quercus robur) — massivt tre" (IFCLABEL)
    SlattSpacingCC_mm = 60. (IFCREAL)
    SlattSpecies_Alternatives = "Eik, Rødeik, Bøk, Ask, Furu, Osp, Bjørk, Gran" (IFCLABEL)
    SlattWidth_mm = 34. (IFCREAL)
    URL = "https://www.assemble.no/assembletile" (IFCLABEL)
    Weight_kg = 3.5899999999999999 (IFCREAL)